# Wiki source code of Announcements

Last modified by Cameron Marx on 2023/08/21 16:47
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all/ none

Legend:
  Created Page
  Modified Extension Page
  Clean Extension Page

Export as HTML

Show last authors

author | version | line-number | content
--- | --- | --- | ---
|  | 1 | (% class="jumbotron" %)
|  | 2 | (((
|  | 3 | (% class="container" %)
|  | 4 | (((
|  | 5 | = Announcements =
|  | 6 |
|  | 7 | Play a [[System Message>>doc:Main.Hive PBX Tutorials.Admin.System Recordings.WebHome]] during you call flow and proceed to the next destination.
|  | 8 | )))
|  | 9 | )))
|  | 10 |
|  | 11 | (% class="row" %)
|  | 12 | (((
|  | 13 | (% class="col-xs-12 col-sm-8" %)
|  | 14 | (((
|  | 15 | == Add/Edit Announcement ==
|  | 16 |
|  | 17 | * **Description**: The name of this announcement
|  | 18 | * **Recording**: Message to be played.
|  | 19 | * **Repeat**:Key to press that will allow for the message to be replayed. If you choose this option there will be a short delay inserted after the message. If a longer delay is needed it should be incorporated into the recording.
|  | 20 | * **Allow Skip**: If the caller is allowed to press a key to skip the message.
|  | 21 | * **Return to IVR**: If this announcement came from an IVR and this box is checked, the destination below will be ignored and instead it will return to the calling IVR. Otherwise, the destination below will be taken. Don't check if not using in this mode. The IVR return location will be to the last IVR in the call chain that was called so be careful to only check when needed. For example, if an IVR directs a call to another destination which eventually calls this announcement and this box is checked, it will return to that IVR which may not be the expected behavior.(% style="display:none" %)
|  | 22 | * **Don't Answer Channel**: Check this to keep the channel from explicitly being answered. When checked, the message will be played and if the channel is not already answered it will be delivered as early media if the channel supports that. When not checked, the channel is answered followed by a 1 second delay. When using an announcement from an IVR or other sources that have already answered the channel, that 1 second delay may not be desired.
|  | 23 |
|  | 24 | == Destination after playback ==
|  | 25 |
|  | 26 | The next step in your call flow.
|  | 27 |
|  | 28 | == Used as Destination ==
|  | 29 |
|  | 30 | What modules point to this Announcement as the destination.
|  | 31 | )))
|  | 32 |
|  | 33 |
|  | 34 | (% class="col-xs-12 col-sm-4" %)
|  | 35 | (((
|  | 36 | {{box title="**Contents**"}}
|  | 37 | {{toc/}}
|  | 38 | {{/box}}
|  | 39 |
|  | 40 | [[~[~[image:ApplicationsAnnouncements.png~|~|alt="ApplicationsAnnouncements.jpg"~]~]>>attach:ApplicationsAnnouncements.png]]
|  | 41 | //Figure 1: Announcements//
|  | 42 | )))
|  | 43 | )))

# Applications

# My Recent Modifications

- Profile of Jonathan Usrey

Axion Communications 2024
For Support Call 855.98AXION or email us at support@axionco.com