# Wiki source code of Directory

Last modified by Cameron Marx on 2023/08/21 16:43
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all/ none

Legend:
  Created Page
  Modified Extension Page
  Clean Extension Page

Export as HTML

Show last authors

author | version | line-number | content
--- | --- | --- | ---
|  | 1 | (% class="jumbotron" %)
|  | 2 | (((
|  | 3 | (% class="container" %)
|  | 4 | (((
|  | 5 | = Directory =
|  | 6 |
|  | 7 | Create Dial-by-Name Directories to allow callers to find their party's extension or for use with IVRs to limit dialable extensions to department members.
|  | 8 | )))
|  | 9 | )))
|  | 10 |
|  | 11 | (% class="row" %)
|  | 12 | (((
|  | 13 | (% class="col-xs-12 col-sm-8" %)
|  | 14 | (((
|  | 15 | == Directory General Options ==
|  | 16 |
|  | 17 | * **Directory Name**: Name of this directory
|  | 18 | * **Directory Description**: Description of this directory
|  | 19 | * **CallerID Name Prefix**: Prefix to be appended to current CallerID Name
|  | 20 | * **Alert Info**: ALERT_INFO to be sent when called from this Directory. Can be used for distinctive ring for SIP devices
|  | 21 |
|  | 22 | == Directory Options (DTMF) ==
|  | 23 |
|  | 24 | * **Announcement**: Greeting to be played on entry to the directory
|  | 25 | * **Invalid Retries**: Number of times to retry when receiving an invalid/unmatched response from the caller
|  | 26 | * **Invalid Retry Recording**: Prompt to be played when an invalid/unmatched response is received, before prompting the caller to try again
|  | 27 | * **Invalid Recording**: Prompt to be played before sending the caller to an alternate destination due to the caller pressing 0 or receiving the maximum amount of invalid/unmatched responses (as determined by Invalid Retries)
|  | 28 | * **Invalid Destination**: Destination to send the call to after Invalid Recording is played
|  | 29 | * **Return to IVR**: When selected, if the call passed through an IVR that had "Return to IVR" selected, the call will be returned there instead of the Invalid destination
|  | 30 | * **Announce Extension**: When checked, the extension number being transferred to will be announced prior to the transfer
|  | 31 |
|  | 32 | == Directory Entries ==
|  | 33 |
|  | 34 | * **Name**: Dialable names that a caller can enter on their dial pad
|  | 35 | * **Name Announcement**: Select recording to use when an entry is matched
|  | 36 | ** **Voicemail Greeting**: User created recording
|  | 37 | ** **Text to Speech**: Automated system reading of "Name" (results may vary)
|  | 38 | ** **Spell Name**: Automated system reading of each letter in "Name"
|  | 39 | ** [[**System Recordings**>>doc:Main.Hive PBX Tutorials.Admin.System Recordings.WebHome]]
|  | 40 | * **Dial**: Destination when entry matched
|  | 41 |
|  | 42 | === ===
|  | 43 | )))
|  | 44 |
|  | 45 |
|  | 46 | (% class="col-xs-12 col-sm-4" %)
|  | 47 | (((
|  | 48 | {{box title="**Contents**"}}
|  | 49 | {{toc/}}
|  | 50 | {{/box}}
|  | 51 |
|  | 52 | [[image:ApplicationsDirectory.png]]
|  | 53 | //Figure 1: Directory//
|  | 54 | )))
|  | 55 | )))

# Applications

Axion Communications 2024
For Support Call 855.98AXION or email us at support@axionco.com